

**BSR/ASHRAE/IES Addendum cc**

 **to ANSI/ASHRAE/IES Standard 90.1-2022**

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Public Review Draft**

Proposed Addendum cc to

Standard 90.1-2022, Energy Standard for Sites and Buildings Except Low-Rise Residential Buildings

**First Public Review (March 2025)**

**(Draft Shows Proposed Changes to Current Standard)**

This draft has been recommended for public review by the responsible project committee. To submit a comment on this proposed standard, go to the ASHRAE website at [www.ashrae.org/standards-research--technology/public-review-drafts](http://www.ashrae.org/standards-research--technology/public-review-drafts) and access the online comment database. The draft is subject to modification until it is approved for publication by the Board of Directors and ANSI. Until this time, the current edition of the standard (as modified by any published addenda on the ASHRAE website) remains in effect. The current edition of any standard may be purchased from the ASHRAE Online Store at [www.ashrae.org/bookstore](http://www.ashrae.org/bookstore) or by calling 404-636-8400 or 1-800-727-4723 (for orders in the U.S. or Canada).

This standard is under continuous maintenance. To propose a change to the current standard, use the change submittal form available on the ASHRAE website, [www.ashrae.org](http://www.ashrae.org).

The appearance of any technical data or editorial material in this public review document does not constitute endorsement, warranty, or guaranty by ASHARE of any product, service, process, procedure, or design, and ASHRAE expressly disclaims such.

© 2025 ASHRAE. This draft is covered under ASHRAE copyright. Permission to reproduce or redistribute all or any part of this document must be obtained from the ASHRAE Manager of Standards, 180 Technology Parkway NW, Peachtree Corners, GA 30092. Phone: 404-636-8400, Ext. 1125. Fax: 404-321-5478. E-mail: standards.section@ashrae.org.

**ASHRAE, 180 Technology Parkway NW, Peachtree Corners, GA 30092**

**© 2025 ASHRAE**

***This draft is covered under ASHRAE copyright. The appearance of any technical data or editorial material in this publication document does not constitute endorsement, warranty, or guaranty by ASHRAE of any product, service, process, procedure, design or the like and ASHRAE expressly disclaims such. Permission to republish or redistribute must be obtained from the MOS.***

**(This foreword is not part of this standard. It is merely informative and does not contain requirements necessary for conformance to the standard. It has not been processed according to the ANSI requirements for a standard and may contain material that has not been subject to public review or a consensus process. Unresolved objectors on informative material are not offered the right to appeal at ASHRAE or ANSI.)**

**FOREWORD**

*This addendum is a routine update to the Section 13 references to ensure the most updated information will be published when the next standard is released in 2025.*

***[Note to Reviewers: This addendum makes proposed changes to the current standard. These changes are indicated in the text by underlining (for additions) and ~~strikethrough~~ (for deletions) except where the reviewer instructions specifically describe some other means of showing the changes. Only these changes to the current standard are open for review and comment at this time. Additional material is provided for context only and is not open for comment except as it relates to the proposed changes.]***

**Addendum cc to 90.1-2022**

**13. NORMATIVE REFERENCES**

**Reference Section**

**Air Conditioning, Heating and Refrigeration Institute (AHRI) 2311 Wilson Blvd., Arlington, VA 22201**

~~AHRI 210/240 (2017) with addendum 1 Unitary Air Conditioning and Air-Source Heat Pump Equipment~~

~~(applicable before 1/1/2023)~~

AHRI 210/240-2023 (2020) Unitary Air Conditioning and Air-Source Heat Pump Equipment

~~(applicable on or after 1/1/2023)~~

~~Table 6.8.1-1,~~

~~Table 6.8.1-2, Table F-1, Table G3.5.1, Table G3.5.2~~

Table 6.8.1-1,

Table 6.8.1-8,

Table 6.8.1-9, Table F-1

AHRI 310/380 (2017) Packaged Terminal Air-Conditioners and Heat Pumps Table 6.8.1-4,

Table G3.5.4

AHRI 340/360 (I-P/2022) Performance Rating of Commercial and Industrial Unitary

Air-Conditioning and Heat Pump Equipment

ANSI/AHRI 365 (~~I-P/2009~~)-2024 (SI/I-P) Commercial and Industrial Unitary Air-Conditioning Condensing

Units

AHRI 390 (I-P/2021) Performance Rating of Single Packaged Vertical Air-Conditioners and Heat Pumps

Table 6.8.1-1,

Table 6.8.1-2, Table G3.5.1, Table G3.5.2

Table 6.8.1-1

Table 6.8.1-4

ANSI/AHRI 400 (I-P/2015) Performance Rating of Liquid-to-Liquid Heat Exchangers 6.4.7

ANSI/AHRI 401 (SI/2015) Performance Rating of Liquid-to-Liquid Heat Exchangers 6.4.7

AHRI 410/2023 (SI/I-P) Performance Rating of Forced-Circulation Air-Cooling

 and Air-Heating Coils Table 6.4.7

AHRI 430 (I-P/2020) Performance Rating of Central Station Air-handling Unit Supply Fans 6.5.3.1.1.2

AHRI 440 (I-P/2019) Performance Rating of Fan-coil Units 6.5.3.1.1.2,

 Table 6.4.7

ANSI/AHRI 460-~~(~~2005~~)~~ (R2024) (SI/I-P) Remote Mechanical Draft Air Cooled Refrigerant Condensers Table 6.8.1-7

AHRI 550/590-~~(I-P/2020)~~2023 (I-P)

~~(with Addendum 1)~~

Performance Rating of Water-Chilling and Heat-Pump Water-Heating Packages Using the Vapor Compression Cycle

6.4.1.2.1, 6.4.1.2.2.1,

6.4.1.2.2.2,

6.4.1.2.2.3,

6.4.1.2.2.4,

Table 6.8.1-3,

Table 6.8.1-16,

Table G3.5.3

AHRI 560 (~~2000~~2023) ~~Absorption Water Chilling and Water Heating Packages~~ Table 6.8.1-3

 Performance Rating of Water-cooled Lithium Bromide

 Absorption Water-chilling and Water-heating Packages

ANSI/AHRI 840-2021 (I-P) Performance Rating of Unit Ventilators Table 6.4.7

 ANSI/AHRI 910 ~~(I-P/2014)~~-2014 (R2023) Performance Rating of Indoor Pool Dehumidifiers Table 6.8.1-12

(I-P)

ANSI/AHRI 920 (I-P/2020 with Addendum 1)

 Performance Rating of DX-Dedicated Outdoor Air System Units 3.2, Table 6.8.1-13,

Table 6.8.1-14

AHRI 1060 (I-P/2018) Performance Rating of Air-to-Air Exchangers for Energy

 Recovery Ventilation Equipment

Table 6.4.7

ANSI/AHRI 1200-2023 ~~(I-P/2013I-P)~~ Performance Rating of Commercial Refrigerated Display

Merchandisers and Storage Cabinets

Table 6.8.1-11,

Table 12.5.1, Table G3.1, Table G3.10.1, Table G3.10.2

6.5.6.1.1.a

6.5.6.1.2.1

ANSI/AHRI 1230-2023 (I-P~~/2014~~)

~~(with Addendum 1)~~

Performance Rating of Variable Refrigerant Flow (VRF) Multi-Split Air-Conditioning and Heat Pump Equipment

Table 6.8.1-8,

Table 6.8.1-9

~~ANSI/AHRI 1230 (I-P/2021) Performance Rating of Variable Refrigerant Flow (VRF) Multi-Split~~

~~Air-Conditioning and Heat Pump Equipment~~

~~Table 6.8.1-8,~~

~~Table 6.8.1-9~~

AHRI Standard 1250 (I-P/2020) Performance Rating of Walk-In Coolers and Freezers Table 6.8.1-20

AHRI Standard 1300-2013 (R2023) Performance Rating of Commercial Heat Pump Water Heaters 11.5.2.3.1

(I-P~~/2013~~)

AHRI Standard 1360-2022 (I-P~~/2017~~) Performance Rating of Computer and Data Processing Room Air

Conditioners

Table 6.8.1-10,

Table 6.8.1-17

**Air Movement and Control Association International (AMCA) 30 West University Drive, Arlington Heights, IL 60004-1806**

ANSI/AMCA 208-18 Calculation of the Fan Energy Index 3.2, 6.5.3.1.3, Table 6.8.1-21

ANSI/AMCA 210-16 Laboratory Methods of Testing Fans for Certified Aerodynamic Performance Rating

ANSI/AMCA 220-21 Laboratory Methods of Testing Air Curtains for Aerodynamic Performance Ratings

ANSI/AMCA Standard 230-~~15~~23 with errata Laboratory Methods of Testing Air Circulating Fans for Rating and

Certification

6.5.3.1.1.2

10.4.5

Table 6.8.1-21

ANSI/AMCA Standard 500-D-18 Laboratory Methods of Testing Dampers for Rating Table 6.4.3.4.3

**~~American Architectural Manufacturers Association (AAMA)~~ Fenestration and Glazing Industry Alliance (FGIA)**

**1900 E. Golf Rd, Suite 1250, Schaumburg, IL 60173-4268**

**Canadian Standards Association (CSA)**

**78 Rexdale Blvd., Toronto, On, Canada M9W 1R3**

**Window and Door Manufacturers Association (WDMA) ~~2025 M Street, NW, Suite 800~~ 2001 K Street, NW, 3rd floor, Washington, DC ~~20036~~20006**

AAMA/WDMA/CSA 101/I.S.2/A440-17(R2022) NAFS-North American Fenestration Standard/Specification for

Windows, Doors, and Skylights

Table 5.8.3.2

**American Iron and Steel Institute (AISI) 25 Massachusetts Avenue, NW, Suite 800**

**Washington, DC 20001**

ANSI/AISI S250-~~20~~21 North American Standard for Thermal Transmittance of Building Envelopes with Cold-Formed Steel Framing

**~~American National Standards Institute (ANSI)~~**

**~~1899 L Street, NW, 11th Floor, Washington, DC 20036~~**

~~A2.5.3, A9.2~~

~~ANSI Z21.47-2021/CSA 2.3-2021 Gas-Fired Central Furnaces Table G3.5.5, Table 6.8.1-5~~

~~ANSI Z83.8-2016/CSA 2.6-2016 (R2021) Gas Unit Heaters, Gas Packaged Heaters, Gas Utility Heaters And~~

~~Gas-Fired Duct Furnaces~~

**American Society of Mechanical Engineers (ASME) Two Park Avenue, New York, NY 10016-5990**

~~Table G3.5.5, Table 6.8.1-5~~

ASME A17.1-~~2019~~2022/CSA B44-16 Safety Code for Elevators and Escalators 10.4.3.3, 10.4.4

**ASHRAE**

**180 Technology Parkway, Peachtree Corners, GA 30092**

ANSI/ASHRAE Standard 51-2016 Laboratory Methods of Testing Fans for Certified Aerodynamic

Performance Rating

Table 6.5.3.7

ANSI/ASHRAE Standard 55-~~2020~~2023 Thermal Environmental Conditions for Human Occupancy Table G3.1 ANSI/ASHRAE Standard 62.1-2022

with addendum ab Ventilation and Acceptable Indoor Air Quality 6.4.3.3.2, 6.4.3.3.5.1,

6.4.3.8, Table 6.4.3.8,

6.5.1, 6.5.2.1, 6.5.2.3,

6.5.3.2.1, 6.5.3.3,

6.5.3.8, 6.5.3.9,

6.5.6.1.2, 6.5.7.1,

11.5.2.2.6, 11.5.2.8.2,

Table 12.5.2-1, G3.2.2.4, G3.2.2.5,

Table L2.2.3 ANSI/ASHRAE Standard 62.2-~~2019~~2022 Ventilation and Acceptable Indoor Air Quality in Residential Buildings 6.5.3.8

ANSI/ASHRAE/IESNA Standard 90.1-2007 Energy Standard for Buildings Except Low-Rise Residential Buildings 6.4.1.2.1

through 2022

ASHRAE Standard 241-2023 Control of Infection Aerosols 6.5.3.8.2

~~ANSI/ASHRAE/IESNA Standard 90.1-2010 Energy Standard for Buildings Except Low-Rise Residential Buildings 6.4.1.2.1~~

~~ANSI/ASHRAE/IESNA Standard 90.1-2013 Energy Standard for Buildings Except Low-Rise Residential Buildings 6.4.1.2.1~~

~~ANSI/ASHRAE/IES Standard 90.1-2016 Energy Standard for Buildings Except Low-Rise Residential Buildings 6.4.1.2.1~~

~~ANSI/ASHRAE/IES Standard 90.1-2019 Energy Standard for Buildings Except Low-Rise Residential Buildings 6.4.1.2.1~~

ANSI/ASHRAE/IES Standard 90.4-~~2019~~2022

~~(with addenda a, b, d, e, and f)~~

Energy Standard for Data Centers 6.6.1, 6.6.2.1, 8.6.1,

Table 11.5.1-1,

11.5.2.2.3

ANSI/ASHRAE Standard 140-~~2020~~2023 Method of Test for Evaluating Building Performance Simulation

Software

12.4.1.4.1,

12.4.1.4.2, 12.7.2,

C2.8, C3.1.4.1,

C3.1.4.2, G1.3.2,

G2.2.4.1, G2.2.4.2,

L3.2.4.1, L3.2.4.2, L3.4

ANSI/ASHRAE Standard 154-~~2016~~2022 Ventilation for Commercial Cooking Operations 6.5.7.2.2

ANSI/ASHRAE Standard 169-2021 Climatic Data for Building Design Standards 5.1. 5.1, 5.1.5.2

ANSI/ASHRAE/ASHE Standard 170-2021 Ventilation of Health Care Facilities 6.4.3.8, 6.5.3.8, 6.5.6.1.2,

Table 11.5.1-1

ANSI/ASHRAE/ACCA Standard 183-~~2007~~

~~(RA 2020)~~2024

Peak Cooling and Heating Load Calculations in Buildings Except Low-Rise Residential Buildings

6.4.2.1

ASHRAE/IES Standard 202-~~2018~~2024 Commissioning Process for Buildings and Systems 4.2.5.2, 4.2.5.2.2

**Association of Home Appliance Manufacturers (AHAM)**

|  |
| --- |
| **1111 19th Street NW, Suite 402, Washington, DC 20036** |
| ANSI/AHAM HRF-1-~~2016~~2019 | Energy and Internal Volume of Refrigerating Appliances | Table G3.10.1 |
| ANSI/AHAM RAC-1-2020 | Room Air Conditioners | Table 6.8.1-4 |
| **ASTM International****100 Barr Harbor Dr., West Conshohocken, PA 19428-2959** |
| ASTM C90-~~16~~24A | Standard Specification for Dry-Cast Loadbearing Concrete Masonry Units | 5.5.3.2, A3.1.1, A9.4.4 |
| ASTM C177-19~~e1~~EO1 | Standard Test Method for Steady-State Heat Flux Measurements and Thermal Transmittance Properties by Means of the Guarded-Hot- Plate Apparatus | A9.3.1 |
| ASTM C272/C272M-18(2024) | Standard Test Method for Water Absorption of Core Materials for Sandwich Constructions | 5.8.1.7.3 |
| ASTM C518-21 | Standard Test Method for Steady-State Thermal Transmittance Properties by Means of the Heat Flow Meter Apparatus | Table 6.8.2, A9.3.1 |
| ASTM C835-06 ~~(2013) e1~~(2020) | Standard Test Method for Total Hemispherical Emittance of Surfaces up to 1400°C | 5.5.3.2.2 |
| ASTM C1224 (2020) | Standard Specification for Reflective Insulation for Building Applications | A9.4.2,Table A9.4.2-2 |
| ASTM C1363-~~19~~24 | Standard Test Method for the Thermal Performance of Building Materials and Envelope Assemblies by Means of a Hot Box Apparatus | A3.3.3.2, A9.3.1, A9.3.2, A10.1 |
| ASTM C1371-15(2022) | Standard Test Method for Determination of Emittance of Materials Near Room Temperature using Portable Emissometers. | 5.5.3.2.2 |
| ASTM C1549-16(2022) | Standard Test Method for Determination of Solar Reflectance Near Ambient Temperature Using a Portable Solar Reflectometer | 5.5.3.2.2 |

ASTM D1003-21 Standard Test Method for Haze and Luminous Transmittance of Transparent Plastics

ASTM E283/E283M-19 Standard Test Method for Determining Rate of Air Leakage through

Exterior Windows, Skylights, Curtain Walls, and Doors Under Specified Pressure Differences Across the Specimen

ASTM E408-13 (2019) Standard Test Methods for Total Normal Emittance of Surfaces Using Inspection-Meter Techniques

ASTM E3158-~~18~~24 Standard Test Method for Measuring the Air Leakage Rate of a Large or Multizone Building

ASTM E779-19 Standard Test Method for Determining Air Leakage Rate by Fan Pressurization

ASTM E972-96 (2021) Standard Test Method for Solar Photometric Transmittance of Sheet Materials Using Sunlight

ASTM E1677-~~19~~23 Standard Specification for an ~~Air Retarder (AR)~~ Barrier (AB) Material or System for Low-Rise Framed Building Walls

ASTM E1680-16(2022) Standard Test Method for Rate of Air Leakage through Exterior Metal Roof Panel Systems

ASTM E1827-~~11 (2017)~~22 Standard Test Methods for Determining Airtightness of Buildings

Using an Orifice Blower Door

ASTM E1980-~~11 (2019)~~24 Standard Practice for Calculating Solar Reflectance Index of Horizontal and Low-Sloped Opaque Surfaces

5.5.4.2.3, 5.5.4.4.2

Table 5.8.3.1, 5.8.3.2

5.5.3.2.2

5.4.3.1.4, 12.5.3, G3.2.1.7

5.4.3.1.4, 12.5.3

5.8.2.6

Table 5.8.3.1

Table 5.8.3.1

5.4.3.1.4, 12.5.3, G3.2.1.7

5.4.3.1.4

ASTM E2178-21a Standard Test Method for Determining Air Leakage Rate and Calculation of Air Permeance of Building Materials

 Table 5.8.3.1

ASTM E2357-~~18~~24 Standard Test Method for Determining Air Leakage Rate of Air Barrier Assemblies

Table 5.8.3.1

ASTM F1361-17 Standard Test Method for Performance of Open Deep Fat Fryers Table 11.5.2.7.2-1

ASTM F1484-18 Standard Test Method for Performance of Steam Cookers Table 11.5.2.7.2-2

ASTM F1495-14a Standard Specification for Combination Oven Electric or Gas Fired Table 11.5.2.7.2-4

ASTM F1496-13 Standard Test Method for Performance of Convection Ovens Table 11.5.2.7.2-4

ASTM F1696-18 Standard Test Method for Energy Performance of Stationary-Rack, Door-Type Commercial Dishwashing Machines

ASTM F1920-15 Standard Test Method for Performance of Rack Conveyor Commercial Dishwashing Machines

Table 11.5.2.7.2-3

Table 11.5.2.7.2-3

ASTM F2093-18 Standard Test Method for Performance of Rack Ovens Table 11.5.2.7.2-4

ASTM F2144-17 Standard Test Method for Performance of Large Open Vat Fryers Table 11.5.2.7.2-1

ASTM F2861-17 Standard Test Method for Enhanced Performance of Combination Oven in Various Modes

Table 11.5.2.7.2-4

**Attachments Energy Rating Council (AERC)**

**355 Lexington Ave., 15th Floor, New York, NY 10017**

AERC-1-~~2021~~2023 Procedures for Determining Energy Performance Properties of Fenestration Attachments

**Cool Roof Rating Council (CRRC)**

**2435 N. Lombard St., Portland, OR 97217, United States**

ANSI/CRRC S100 (~~2021~~2025) Standard Test Methods for Determining Radiative Properties of

Materials

Table 12.5.1

Table G3.1

5.5.3.1.4

**CSA Group**

**178 Rexdale Blvd., ~~Toronto, ON, Canada, M9W 1R3~~ Etobicoke/Toronto, ON or under the US Headquarters at 5801 E. Pleasant Valley Rd., Independence, OH 44131**

CSA C439-2018 (R2022) Laboratory Methods of Test for Rating the 6.4.7

Performance of Heat/Energy-Recovery Ventilators 6.5.6.1.1.b

ANSI Z21.47-2021/CSA 2.3-2021 Gas-Fired Central Furnaces Table G3.5.5,

 Table 6.8.1-5

ANSI Z83.8-2016/CSA 2.6-2016 (R2021) Gas Unit Heaters, Gas Packaged Heaters, Gas Utility Heaters And Table G3.5.5, Gas-Fired Duct Furnaces Table 6.8.1-5

**Cooling Technology Institute (CTI)**

**~~3845 Cypress Creek Parkway, Suite 420, Houston, TX 77068;~~ 13231 Champion Forest Drive, Suite 230, Houston, TX 77069; P.O. Box 681807, Houston, TX 77268**

CTI ATC-105 (~~19~~22) Acceptance Test Code for Water Cooling Towers Table 6.8.1-7

CTI ATC-105 Adiabatic (23) Acceptance Test Code for Adiabatic Fluid Coolers Table 6.8.1-7

CTI ATC-105DS (18) Acceptance Test Code for Dry Fluid Coolers Table 6.8.1-7

CTI ATC-105S (11) Acceptance Test Code for Closed-Circuit Cooling Towers Table 6.8.1-7

CTI ATC-106 (11) Acceptance Test Code for Mechanical Draft Evaporative Vapor Condensers

Table 6.8.1-7

CTI STD-201 RS (21) Performance Rating of Evaporative Heat Rejection Equipment Table 6.8.1-7

**Door and Access Systems Manufacturers Association (DASMA) 1300 Sumner Avenue, Cleveland, OH 44115-2851**

ANSI/DASMA 105-2020 Test Method for Thermal Transmittance and Air Infiltration of Garage Doors and Rolling Doors

**International Association of Plumbing and Mechanical Officials (IAPMO) 4755 E. Philadelphia Street, Ontario, CA 91761-2816**

5.8.3.2,

Table 5.8.3.2

IAPMO/ANSI WE·Stand-~~2017~~2023 Water Efficiency and Sanitation Standard for the Built Environment 11.5.2.3.5

**International Organization for Standardization (ISO) ISO Central Secretariat BIBC II Chemin de Blandonnet 8, CP 401, 1214, Vernier, Geneva, Switzerland**

|  |  |  |
| --- | --- | --- |
| ISO 5801:2017ISO 9050 (2003) | Fans—Performance Testing Using Standardized AirwaysGlass in Building—Determination of Light Transmittance, Solar Direct Transmittance, Total Solar Energy Transmittance, Ultraviolet Transmittance and Related Glazing Factors | 6.5.3.1.1.25.5.3.2.2 |
| ISO 10211 (2017) | Thermal bridges in building construction—Heat flows and surface temperatures—Detailed calculations | A10.1 |
| ANSI/AHRI/ASHRAE/ISO 13256-1:1998(2021) | Water-Source Heat Pumps—Testing and Rating for Performance— Part 1: Water-to-Air and Brine-to-Air Heat Pumps | Table 6.8.1-15 |
| ANSI/AHRI/ASHRAE/ISO 13256-2:1998(2021) | Water-Source Heat Pumps—Testing and Rating for Performance— Part 2: Water-to-Water and Brine-to-Water Heat Pumps | Table 6.8.1-15 |
| ISO 14683 (2017) | Thermal bridges in building construction—Linear thermal transmittance—Simplified methods and default values | A10.1 |
| ISO 25745-2:2015 | Energy Performance of Lifts, Escalators and Moving Walks—Part 2: | 10.4.3.4, 10.9.3, |
|  | Energy Calculation and Classification for Lifts (Elevators) | 11.5.2.7.1 |

**National Electrical Manufacturers Association (NEMA) 1300 N. 17th Street, Suite 900, Arlington, VA 22209**

ANSI/NEMA MG 1-~~2016, with 2021~~2024

~~Revisions~~

Motors and Generators 3.2

**National Fenestration Rating Council (NFRC)**

**6305 Ivy Lane, Suite 140, Greenbelt, MD 20770-6323**

ANSI/NFRC 100-~~2020~~2023 Procedure for Determining Fenestration Product U-Factors 5.8.2.4

ANSI/NFRC 200-~~2020~~2023 Procedure for Determining Fenestration Product Solar Heat Gain Coefficients and Visible Transmittance at Normal Incidence

ANSI/NFRC 203-~~2020~~2023 Procedure for Determining Visible Transmittance of Tubular Daylighting Devices

NFRC 300-~~2020~~2023 Test Method for Determining the Solar Optical Properties of Glazing Materials and Systems

5.5.4.6, 5.8.2.5

5.8.2.6

5.8.2.6

5.8.2.6

NFRC 301-~~2020~~2023 Standard Test Method for Emittance of Glazing Products 5.5.4.6

ANSI/NFRC 400-~~2020~~2023 Procedure for Determining Fenestration Product Air Leakage Table 5.8. 3.2, 5.8.3.2

**National Fire Protection Association (NFPA)**

**1 Battery March Park, Quincy, MA 02269-9101; P.O. Box 9101**

NFPA 70-~~2020~~2023 National Electric Code 6.5.1, 8.4. 3.1, 8.4.3.2

NFPA 96-~~2021~~2024 Ventilation Control and Fire Protection of Commercial Cooking Operations

G3.2.2.9

**Telecommunications Industry Association (TIA)**

|  |  |  |
| --- | --- | --- |
| **1320 North Courthouse Road, Suite 200** |  |  |
| ANSI/TIA-942-~~REV B~~C, ~~July 12, 2017~~2024 | Telecommunication Infrastructure Standard for Data Centers | 6.5.1 |
| **UL, LLC****333 Pfingsten Rd., Northbrook, IL 60062** |  |  |
| UL 181A-2021 | Closure Systems for Use with Rigid Air Ducts and Air Connectors | 6.4.4.2.1 |
| UL 181B-2021 | Closure Systems for Use with Flexible Air Ducts and Air Connectors | 6.4.4.2.1 |
| UL 727-~~2018~~2024 | UL Standard for Safety—Oil Fired Central Furnaces | Table 6.8.1-5 |
| UL 731-2021 | UL Standard for Safety—Oil-Fired Unit Heaters | Table 6.8.1-5 |
| **U.S. Department of Defense****3010 Defense Pentagon, Washington, DC 20301** |
| MIL-P-17639F (~~1996~~2017) | Pumps, Centrifugal, Miscellaneous Service, Naval Shipboard Use | 10.4.8 |
| MIL-P-17840~~C~~D (~~1986~~2018) | Pumps, Centrifugal, Close-Coupled, Navy Standard (for Surface Ship Application) | 10.4.8 |
| MIL-P-17881D (1972) | Pumps, Centrifugal, Boiler Feed (Multi-Stage) | 10.4.8 |
| ~~MIL-P-18472G (1989)~~ | ~~Pumps, Centrifugal, Condensate, Feed Booster, Waste Heat Boiler, and Distilling Plant~~ | ~~10.4.8~~ |
| ~~MIL-P-18682D~~ | ~~Pump, Centrifugal, Main Condenser Circulating, Naval Shipboard~~ | ~~10.4.8~~ |

**U.S. Department of Energy (DOE)**

**1000 Independence Avenue, SW, Washington, DC 20585**

10 CFR Part 430 Subpart B, App N Uniform Test Method for Measuring the Energy Consumption of

Furnaces Other Than Boilers

10 CFR Part 430, Subpart B App U Uniform Test Method for Measuring the Energy Consumption of

Ceiling Fans

~~10 CFR Part 430 Subpart B App U Uniform Test Method for Measuring the Energy Consumption of~~

~~Ceiling Fans~~

10 CFR Part 431.304 Uniform Test Method for the Measurement of Energy Consumption of Walk-In Coolers and Walk-In Freezers

10 CFR 431 Subpart K, App A Uniform Test Method for Measuring the Energy Consumption of

Distribution Transformers

10 CFR Part 431, Subpart B, App B Uniform Test Method for Measuring ~~Nominal Full-Load~~ the Efficiency of Electric Motors

10 CFR Part 431, Subpart Y Pumps: Definitions, Energy Conservation Standards, and Uniform

Test Method of the Measurement of Energy Consumption of Pumps

Table 6.8.1-5,

Table 6.8.1-6, Table F-4

6.5.3.7,

Table 6.8.1-21,

F3, Table F-6 ~~F3~~

42 USC 6831, et seq., Public Law 102-486 Energy Policy Act of 1992, EPACT 2005, and EISA 2007 6.4.1.1

**~~U.S. Security and Exchange Commission (SEC) 100 F Street, NE, Washington, DC 20549~~**

The Interagency Paper on Sound Practices to Strengthen the Resilience of the US Financial System

The interagency Paper on Sound Practices to Strengthen the Resilience of the US Financial System, April 7, 2003

Exemptions to 6.5.1

**16 INFORMATIVE APPENDIX e INFORMATIVE REFERENCES**

ASTM E2813-~~18~~24 Standard Practice for Building Enclosure Commissioning 5.9.1, H1

[ . . . ]

Revised Table G3.1 to accommodate the normative reference update to ASHRAE Standard 55

1. **Schedule**

|  |  |
| --- | --- |
| Schedules capable of modeling hourly variations in occupancy, lighting power, miscellaneous *equipment* power, *thermostat set points*, and *HVAC system* operation shall be used. The schedules shall be typical of the proposed *building* type as determined by the designer and approved by the *rating authority*.**Temperature and Humidity Schedules.** Temperature and humidity control *set points* and schedules as well as *temperature control throttling range* shall be the same for *proposed design* and *baseline building design*.**HVAC System Fan Schedules.** Schedules for *HVAC system* fans that provide *outdoor air* for *ventilation* shall run continuously whenever *spaces* are occupied and shall be cycled ON and OFF to meet heating and cooling loads during unoccupied hours.**Exceptions:**1. Where no heating and/or cooling *system* is to be installed, and a heating or cooling *system* is being simulated only to meet the requirements described in this table, heating and/or cooling *system* fans shall not be simulated as running continuously during occupied hours but shall be cycled ON and OFF to meet heating and cooling loads during all hours.
2. *HVAC system* fans shall remain on during occupied and unoc- cupied hours in *spaces* that have health- and safety-mandated minimum *ventilation* requirements during unoccupied hours.
3. *HVAC system* fans shall remain on during occupied and unoc- cupied hours in *systems* primarily serving *computer rooms*.
4. Dedicated *outdoor air* supply fans shall stay off during unoc- cupied hours.
 | Same as *proposed design.***Exceptions:**1. *Set points* and schedules for *HVAC systems* that *automati- cally* provide occupant thermal comfort via means other than directly controlling the air dry-bulb and wet-bulb tempera- ture may be allowed to differ, provided that equivalent levels of occupant thermal comfort are demonstrated via the meth- odology in ASHRAE Standard 55, Section ~~5.3.3~~5.3.4, “Elevated Air Speed,” or Standard 55, Appendix B, “Computer Pro- gram for Calculation of PMV-PPD.”
2. When the proposed *building* design includes *HVAC systems* serving *dwelling units* or *sleeping units* that have controls meeting requirements of Section 11.5.2.2.4 “H04: Residential Space HVAC Control”:
	1. The *baseline building design* shall be modeled using heating temperature setback of 5°F (3°C) higher than in the *proposed design* but not higher than the occupied temperature for a maximum of 9 hours per day.
	2. The *baseline building design* shall be modeled using cooling temperature setback of 5°F (3°C) lower than the *proposed design* but not lower than the occupied temperature for not more than 9 hours per day.
3. Schedules may be allowed to differ between *proposed design* and *baseline building design* when necessary to model non- standard *efficiency* measures, provided that the revised schedules have been approved by the *rating authority*. Mea- sures that may warrant use of different schedules include but are not limited to *automatic* lighting controls, *automatic* nat- ural *ventilation* controls, *automatic demand control ventila- tion* controls, and *automatic* controls that reduce *service water-heating* loads. In no case shall schedules differ where the controls are *manual* (e.g., *manual* operation of light switches or *manual* operation of windows).
4. *HVAC system* fan schedules may be allowed to differ when Section G3.2.1.2(a) applies.
5. For *Systems* 6 and 8, only the *terminal*-unit fan and *reheat* coil shall be energized to meet heating *set point* during unoc- cupied hours
6. Lighting schedules may be allowed to differ based on occupancy sensor reduction factor in Tables G3.7-1 and G3.7-2.
 |